**Copper tails**

M11 X 1, L. 337mm

2 per pack

Reference: **811611.2P**

Specification description

Soft-tempered copper tails Ø M11 X 1, L. 337mm to supply mixers and taps.

Can be installed instead of PEX flexibles.

Improves efficiency of thermal shocks.

Supplied in packs of 2.

Pro tip: Don't forget to include non-return valves on the copper tails if the PEX flexibles to be replaced have integral non-return valves. Call our Technical Team for more information.