**Push-fit BIOFIL connector M24/125**

For wall-mounted fixed showers or shower panels

Reference: **820125**

Specification description

Push-fit connector M24/125 for wall-mounted fixed showers or shower panels.

For quick and easy installation of filtration devices on wall-mounted showers or a DELABIE shower panel (SPORTING, SECURITHERM, etc.).

30-year warranty.